!PADS-POWERPCB-V9.0-METRIC-CP949! NETLIST FILE FROM PADS LOGIC VVX.2
*REMARK* 20305 VB0HW0100.sch -- Mon Mar 09 17:28:45 2026
*REMARK*  


*PCB*        GENERAL PARAMETERS OF THE PCB DESIGN

MAXIMUMLAYER 4              Maximum routing layer

*PART*       ITEMS
R31     RES1005@1005
C17     CAP1005@1005
U2      OPA2836IDGSR@SOP50P490X110-10N
C18     CAP1005@1005
J2      2026560021@2026560021
R23     RES1005@1005
R8      RES1005@1005
U9      RECE.20279.001E.01@RECE.20279.001E.01
R11     RES1005@1005
C2      CAP1005@1005
C30     CAP1608@1608
C4      CAP1005@1005
R25     RES1005@1005
J4      217B-CA04@ATTEND_217B-CA04
J1      ECV3-06-ICESPI@ECV3-06-ICESPI
C19     CAP1005@1005
C16     CAP1005@1005
C23     CAP1005@1005
R28     RES1005@1005
R42     RES1005@1005
R6      RES1005@1005
R12     RES1005@1005
U5      MIC5528-3.3YMT@MIC5528-3.3YMT
C21     CAP1005@1005
C22     CAP1005@1005
C31     CAP1005@1005
R14     RES1005@1005
LED3    LED1608@LED1608
C32     CAP1608@1608
C20     CAP1005@1005
R16     RES1005@1005
R18     RES1005@1005
U20     PESD5V0F1BLD_315@PESD5V0F1BLD315
C15     CAP1005@1005
C24     CAP1005@1005
C5      CAP1608@1608
C7      CAP1608@1608
C10     CAP1608@1608
C14     CAP1005@1005
C12     CAP1005@1005
C13     CAP1608@1608
C37     CAP1608@1608
C38     CAP1608@1608
U23     ADL5513ACPZ-R7@QFN50P300X300X80-17N-D
C61     CAP1005@1005
R19     RES1005@1005
R29     RES1005@1005
C64     CAP1005@1005
C67     CAP1005@1005
R20     RES1005@1005
C72     CAP1005@1005
C29     CAP1608@1608
L4      IND1608@1608
L3      IND1005@1005
Y1      FC-12M@FC-12M
R26     RES1005@1005
R27     RES1005@1005
Y2      FA-128_32MHZ@FA-128
R35     RES1005@1005
C51     CAP1005@1005
L1      IND1608@1608
C42     CAP1608@1608
C36     CAP1005@1005
R24     RES1005@1005
H2      M2_HOLE@HOLE-1.8
C43     CAP1608@1608
C39     CAP1608@1608
T5      TEST_POINT@TP
H3      M2_HOLE@HOLE-1.8
C28     CAP1005@1005
C27     CAP1005@1005
R36     RES1005@1005
C26     CAP1005@1005
C25     CAP1005@1005
R39     RES1005@1005
C40     CAP1005@1005
C41     CAP1005@1005
C44     CAP1608@1608
C45     CAP1608@1608
C46     CAP1608@1608
C47     CAP1608@1608
C48     CAP1005@1005
C49     CAP1005@1005
U16     W25Q32RVXHJQ_TR@SON50P300X200X40-9N
C50     CAP1608@1608
C103    CAP1005@1005
R83     RES1005@1005
C52     CAP1608@1608
R30     RES1005@1005
C34     CAP1005@1005
R40     RES1005@1005
L5      IND1005@1005
U6      PRG18BC1R0MM1RB@THRMC1608X95N
U7      PRG18BC1R0MM1RB@THRMC1608X95N
L6      IND1608@1608
SW2     A03-05@A03-05
C53     CAP1005@1005
R17     RES1005@1005
R41     RES1005@1005
C54     CAP1005@1005
C55     CAP1005@1005
C56     CAP1608@1608
R43     RES1005@1005
LED4    LED1608@LED1608
U4      PMFPB8032XP@PMFPB8032XP
P1      AXT510124@PANASONIC_AXT510124
R15     RES1005@1005
H4      M2_HOLE@HOLE-1.8
U10     ICM-42670-P@ICM-42675-P
U27     MD1822K6-G@QFN50P300X300X100-17N-D
C35     CAP1005@1005
C8      CAP1608@1608
C9      CAP1005@1005
H1      M2_HOLE@HOLE-1.8
JP1     TP_DBL@TP_DBL
R65     RES1005@1005
D3      DAP222WM@EMD3F-DAP222WM
D4      BAS3005B-02V@SC79-BAS3005B-02V
U1      PRTR5V0U2X@SOT143B-PRTR5V0U2X
R34     RES1005@1005
U22     TMP235-Q1@SOT-23
L2      IND1608@1608
R21     RES1005@1005
R22     RES1005@1005
U8      SN74LVC1G04DRY2@USON-SN74LVC1G04DRY2
R33     RES1005@1005
R32     RES1005@1005
R37     RES1005@1005
R4      RES1005@1005
U30     TC7920K6-G@SON50P400X400X100-13N-D
R38     RES1005@1005
C62     CAP1005@1005
C65     CAP1005@1005
C70     CAP1005@1005
C74     CAP1005@1005
U26     NRF52840_QIAA_R@NRF52840-QIAA-F-R7
U3      MCP73838@MSOP10-MCP73838
C73     CAP1005@1005
C11     CAP1608@1608
C75     CAP1005@1005
U31     MAX14778ETP+@QFN65P500X500X80-21N
C76     CAP1005@1005
C77     CAP1005@1005
R58     RES1005@1005
C33     CAP1608@1608
R73     RES1005@1005
R63     RES1005@1005
U34     MD0100N8-G@AMP_PHA-1
C80     CAP1005@1005
C81     CAP1005@1005
PZT_PE  TEST_POINT@TP
PZT_DMP TEST_POINT@TP
PZT_PIN TEST_POINT@TP
PZT_NIN TEST_POINT@TP
C82     CAP1005@1005
C83     CAP1005@1005
PZT_T/R TEST_POINT@TP
C84     CAP1005@1005
L10     IND1608@1608
L11     IND1608@1608
L12     IND1608@1608
L14     IND1608@1608
C1      CAP1608@1608
U32     LT3463EDDPBF@DFN-10_DD
C3      CAP1608@1608
C6      CAP1608@1608
R7      RES1005@1005
L13     IND1608@1608
R10     RES1005@1005
R9      RES1005@1005
R5      RES1005@1005
L15     IND1608@1608
TH1     THER1608@TH1608-NB21K00103KBB
R13     RES1005@1005
C85     CAP1005@1005
C86     CAP1005@1005
D1      B0540WS-TP@SOD2512X115N
R66     RES1005@1005
R67     RES1005@1005
C87     CAP1005@1005
R68     RES1005@1005
R69     RES1005@1005
R70     RES1005@1005
R71     RES1005@1005
C88     CAP1005@1005
C89     CAP1005@1005
C79     CAP1005@1005
L16     IND1608@1608
U33     MCP1804T-A002I_OT@SOT95P270X145-5N
C90     CAP1005@1005
C91     CAP1005@1005
C98     CAP1005@1005
R1      RES1005@1005
R2      RES1005@1005
LED1    LED1608@LED1608
LED2    LED1608@LED1608
L17     IND1608@1608
R3      RES1005@1005
R74     RES1005@1005
C110    CAP1005@1005
R77     RES1005@1005
C119    CAP1005@1005
R79     RES1005@1005
R80     RES1005@1005
U37     ADC121S051CIMF_NOPB@SOT95P280X145-6N
C78     CAP1005@1005
C93     CAP1005@1005
C95     CAP1005@1005
T1      TEST_POINT@TP
T2      TEST_POINT@TP
T3      TEST_POINT@TP
L19     IND1608@1608
U38     LM27762DSSR@SON50P200X300X80-13N-D
U42     MIC5528-3.3YMT@MIC5528-3.3YMT
C96     CAP1005@1005
R64     RES1005@1005
R72     RES1005@1005
R76     RES1005@1005
R78     RES1005@1005
R81     RES1005@1005
L20     IND1608@1608
R82     RES1005@1005
L22     IND1608@1608
L23     IND1608@1608
C102    CAP1005@1005
U41     MIC5528-3.3YMT@MIC5528-3.3YMT
C104    CAP1608@1608
L32     IND1608@1608
R61     RES1005@1005
C121    CAP1005@1005
R84     RES1005@1005
C105    CAP1005@1005
R87     RES1005@1005
C106    CAP1005@1005
T4      TEST_POINT@TP
T6      TEST_POINT@TP
CS      TEST_POINT@TP
MISO    TEST_POINT@TP
SCLK    TEST_POINT@TP
R90     RES1005@1005
C109    CAP1005@1005
C113    CAP1608@1608
L31     IND1608@1608
C114    CAP1005@1005
C115    CAP1608@1608
C116    CAP1608@1608
*NET*
*SIGNAL* 2NDAMP_IN
C78.1 U2.7 R82.2 
*SIGNAL* $$$21938
U31.1 R11.2 
*SIGNAL* $$$26420
C51.2 U23.4 U23.1 L1.1 C42.1 
*SIGNAL* 2NDAMP_OUT
U2.9 R80.2 T4.1 C40.2 
*SIGNAL* GND
C16.2 C17.2 C18.1 Y2.4 Y2.2 
C21.1 C22.1 C28.1 C19.1 U26.B7 
C20.1 C31.1 C24.1 C29.2 C30.2 
C32.2 C36.1 C26.1 C14.1 C25.1 
U26.F23 C27.1 U10.7 U10.6 C34.1 
C33.2 C35.1 U10.1 U10.2 U10.3 
U10.10 U10.11 J1.5 C72.1 C73.1 
U9.1 U9.2 C15.1 U26.74 U16.4 
U16.9 C53.1 R41.2 C11.2 U5.3 
C8.2 R17.2 C9.2 R15.2 R21.2 
U5.5 U3.5 TH1.2 R7.2 R13.2 
R10.2 C6.2 C1.2 J2.2 U1.1 
C3.2 R29.1 C23.1 C121.1 R4.2 
C65.1 U22.3 C119.1 J4.A1/B12 J4.A12/B1 
J4.SH2 J4.SH1 R37.2 R38.2 U27.17 
U27.3 U27.6 U27.7 U27.14 U30.12 
U30.9 U30.13 U31.3 C77.1 C82.2 
C48.1 C76.1 C84.1 C85.2 U32.11 
R71.2 C88.2 C89.2 U33.2 C90.2 
C91.2 C79.2 C104.2 U42.3 R65.2 
C98.2 U42.5 C114.2 C115.2 C81.1 
C80.1 C38.2 C47.2 C83.2 C49.1 
R6.2 P1.8 P1.4 P1.7 P1.3 
U41.3 C113.2 U41.5 C116.2 R77.1 
R79.1 U37.2 C95.1 U38.13 C10.2 
R76.1 R81.2 U38.4 C52.2 C7.2 
C5.2 C102.1 R83.2 C105.2 C106.2 
C109.2 R3.1 C93.1 R82.1 C4.1 
C2.1 U20.2 C12.1 C13.2 C37.2 
U23.17 C64.1 U23.10 U23.5 U23.6 
U23.7 U23.8 U23.16 U23.15 U23.13 
C67.2 R26.2 R27.1 C51.1 C39.2 
R36.2 C41.2 C42.2 C43.2 C44.2 
C45.2 C46.2 C50.2 C54.1 C55.1 
C56.2 J2.3 J2.4 U5.7 U8.3 
U3.11 U42.7 
*SIGNAL* PREAMP_OUT
R74.2 C103.2 T2.1 U2.1 
*SIGNAL* SWDIO
U26.AC24 J1.2 
*SIGNAL* INT2_ICM
U26.G1 R31.2 U10.9 
*SIGNAL* SWDCLK
U26.AA24 J1.4 
*SIGNAL* $$$7457
U23.2 C61.1 
*SIGNAL* $$$3365
R43.2 LED4.1 
*SIGNAL* $$$7588
R19.2 R20.1 U23.12 
*SIGNAL* $$$4037
J4.A4/B9 U6.1 J4.A9/B4 
*SIGNAL* $$$3654
U42.2 L32.1 U42.1 
*SIGNAL* PWR_MCU_EN
R17.1 U5.4 C9.1 R22.2 D3.1 
*SIGNAL* $$$14862
C64.2 U23.14 
*SIGNAL* \SPI_CS_LOCK-IN
U26.AD8 
*SIGNAL* SYNCO
U26.AD12 
*SIGNAL* ADC_RDATA_N
U26.B13 
*SIGNAL* ADC_RDATA_P
U26.A12 
*SIGNAL* XL1
C16.1 Y1.2 U26.D2 
*SIGNAL* I2C_SCL_ICM
U26.B15 U10.13 R34.2 
*SIGNAL* XL2
C17.1 Y1.1 U26.F2 
*SIGNAL* $$$25958
L3.2 U26.E24 C14.2 C15.2 U26.B5 
*SIGNAL* VDD_BAT
C6.1 J2.1 U3.10 U4.4 R28.2 
*SIGNAL* $$$22393
R90.2 C109.1 U38.12 U38.8 
*SIGNAL* SPI_SCK
U26.AC9 U16.6 R18.1 
*SIGNAL* $$$32490
R23.2 LED3.1 
*SIGNAL* $$$15263
U23.3 C67.1 
*SIGNAL* SPI_MOSI
U26.AC11 U16.5 
*SIGNAL* VBUS_IN
U1.4 L2.1 U6.2 
*SIGNAL* $$$15328
R20.2 R26.1 U23.11 
*SIGNAL* $$$24450
U3.8 R5.2 R10.1 
*SIGNAL* $$$20152
R35.1 R27.2 U23.9 
*SIGNAL* RXD
U26.M2 J1.6 
*SIGNAL* TXD
U26.L1 J1.3 
*SIGNAL* $$$16529
U26.H23 C25.2 L5.2 
*SIGNAL* ADC_TEMP
U26.K2 U22.2 C119.2 
*SIGNAL* I2C_SCL_NIR
U26.L24 R25.1 
*SIGNAL* PWR_HOLD
U26.N1 D4.2 
*SIGNAL* I2C_SDA_NIR
U26.J24 R24.1 
*SIGNAL* $$$22557
CS.1 U37.6 R8.2 R14.2 
*SIGNAL* VBUS
U4.5 JP1.2 R15.1 U3.1 U3.7 
R5.1 C1.1 LED2.2 LED1.2 L2.2 
*SIGNAL* SPI_MISO
U26.AD10 U16.2 R16.1 
*SIGNAL* $$$5070
U4.3 U4.6 U4.7 U4.8 U7.1 
*SIGNAL* INT1_ICM
U10.4 R32.2 U26.A16 
*SIGNAL* $$$22594
MISO.1 U37.5 R16.2 
*SIGNAL* $$$6539
L4.2 L3.1 
*SIGNAL* $$$12824
R19.1 R87.2 
*SIGNAL* ANT
C26.2 U9.3 L5.1 C28.2 C27.2 
*SIGNAL* $$$12989
R36.1 R39.2 C40.1 
*SIGNAL* $$$3572
U27.16 U27.1 PZT_DMP.1 R12.2 
*SIGNAL* $$$25431
U26.C1 C18.2 
*SIGNAL* $$$6537
L4.1 U26.B3 
*SIGNAL* VCC_NRF
C32.1 U26.AD2 
*SIGNAL* $$$22610
SCLK.1 U37.4 R18.2 
*SIGNAL* $$$12990
R39.1 C41.1 T5.1 C61.2 
*SIGNAL* I2C_SDA_ICM
U26.A14 U10.14 R33.2 
*SIGNAL* $$$85
U3.2 C3.1 
*SIGNAL* $$$1313
U3.6 R7.1 
*SIGNAL* \WP_FLASH
U26.H2 U16.3 R41.1 
*SIGNAL* $$$18796
R38.1 J4.B5 
*SIGNAL* $$$18801
R37.1 J4.A5 
*SIGNAL* $$$1329
TH1.1 R13.1 R9.2 
*SIGNAL* $$$16790
R9.1 U3.9 
*SIGNAL* $$$3604
U27.5 PZT_NIN.1 R40.2 
*SIGNAL* $$$3606
U27.4 PZT_PIN.1 R30.2 
*SIGNAL* ADC_BAT
U26.J1 R28.1 R29.2 C23.2 
*SIGNAL* VDD_MAIN
SW2.1 C8.1 U7.2 U5.6 U42.6 
C115.1 U41.6 C116.1 C54.2 
*SIGNAL* $$$26274
U26.N24 C24.2 
*SIGNAL* PZT_EN_MUXB
U26.AC19 U31.16 
*SIGNAL* \SPI_CS_FLASH
U26.AD20 R42.1 U16.1 
*SIGNAL* $$$20341
JP1.1 U4.1 
*SIGNAL* $$$18101
R61.1 C121.2 D3.3 
*SIGNAL* PWR_I/R_EN
U26.T2 
*SIGNAL* LIGHT_ON
U26.AD18 
*SIGNAL* $$$27542
U26.AC5 C30.1 
*SIGNAL* $$$18102
D3.2 U8.2 R21.1 
*SIGNAL* BUTTON_CHECK
U26.P2 U8.4 
*SIGNAL* $$$18103
R22.1 D4.1 
*SIGNAL* LED_BLE
U26.U1 R23.1 
*SIGNAL* NIRLED_SEL0
U26.U24 
*SIGNAL* NIRLED_SEL1
U26.T23 
*SIGNAL* $$$4032
U5.2 U5.1 L6.1 
*SIGNAL* GND_RX
U41.7 
*SIGNAL* $$$14845
U26.D23 C72.2 
*SIGNAL* $$$14940
C73.2 U26.A18 
*SIGNAL* $$$3432
R61.2 R4.1 SW2.2 
*SIGNAL* FUNCTION_LED
U26.A10 R43.1 
*SIGNAL* $$$20788
L23.1 U2.4 C102.2 C37.1 
*SIGNAL* ADC_PRESSURE
U26.A8 
*SIGNAL* $$$14839
U27.8 C62.1 
*SIGNAL* $$$14847
C62.2 U30.5 
*SIGNAL* +3.3V_M
C19.2 U26.A22 U26.AD23 C29.1 U26.Y2 
R25.2 U26.AD14 C33.1 C35.2 R33.1 
R34.1 R32.1 U10.12 C34.2 U10.5 
R31.1 R24.2 J1.1 U10.8 C20.2 
U26.B1 C31.2 U26.W1 C36.2 U16.7 
U16.8 C53.2 R42.2 L6.2 C11.1 
LED3.2 LED4.2 U8.6 
*SIGNAL* STAT1_1
R1.2 U3.3 
*SIGNAL* STAT1_2
U3.4 R2.2 
*SIGNAL* $$$30190
R1.1 LED1.1 
*SIGNAL* $$$30191
R2.1 LED2.1 
*SIGNAL* $$$14861
C70.1 U27.9 
*SIGNAL* NIR_WAV_SEL0
U26.Y23 
*SIGNAL* $$$14864
C70.2 U30.3 
*SIGNAL* $$$14885
U27.12 C74.1 
*SIGNAL* $$$14887
C74.2 U30.2 
*SIGNAL* ADC_AGC
U26.B9 
*SIGNAL* AGC_SW
U26.AD16 
*SIGNAL* $$$14896
U27.13 C75.1 
*SIGNAL* $$$14902
C75.2 U30.1 
*SIGNAL* $$$25289
U30.6 C82.1 L11.1 C48.2 
*SIGNAL* PZT_-20V
L12.2 D1.A R68.1 C89.1 
*SIGNAL* $$$25231
U27.10 U27.11 L10.1 U27.2 C81.2 
C80.2 
*SIGNAL* PZT_PE
U26.AC21 U27.15 R6.1 PZT_PE.1 
*SIGNAL* PZT_DMP
U26.AD22 R12.1 
*SIGNAL* PZT_P_PULSE
U26.P23 R30.1 
*SIGNAL* PZT_N_PULSE
U26.R24 R40.1 
*SIGNAL* $$$2625
U31.2 C77.2 
*SIGNAL* PD_SEL0
U26.B17 
*SIGNAL* $$$2626
U31.4 U31.21 C76.2 
*SIGNAL* $$$2708
U30.11 U30.8 U30.10 R58.1 U30.7 
*SIGNAL* PZT_RX
R58.2 PZT_T/R.1 U31.5 R11.1 U34.1 
*SIGNAL* $$$25617
L22.1 U2.10 U2.5 U2.6 C93.2 
C13.1 
*SIGNAL* $$$24188
R3.2 U2.2 R74.1 
*SIGNAL* $$$24714
R77.2 T1.1 C110.1 U2.3 
*SIGNAL* PD_SEL1
U26.B19 
*SIGNAL* $$$5663
U34.3 U20.1 C110.2 
*SIGNAL* $$$7726
R79.2 U2.8 R80.1 
*SIGNAL* $$$6258
U31.9 P1.6 
*SIGNAL* $$$6259
U31.8 P1.5 
*SIGNAL* $$$6260
U31.7 P1.2 
*SIGNAL* PZT_CH_SEL1
U26.B11 U31.14 U31.12 
*SIGNAL* PZT_CH_SEL0
U26.A20 U31.15 U31.11 
*SIGNAL* $$$6261
U31.6 P1.1 
*SIGNAL* PZT_EN_MUXA
U26.AC17 U31.10 
*SIGNAL* PZT_+10V
L10.2 U33.5 C91.1 
*SIGNAL* PZT_+20V
L11.2 U32.1 R69.1 C88.1 L17.1 
*SIGNAL* $$$6264
U31.19 P1.10 
*SIGNAL* $$$6265
U31.20 P1.9 
*SIGNAL* $$$13633
U33.4 C79.1 R73.2 
*SIGNAL* NIR_WAV_SEL1
U26.W24 
*SIGNAL* NIR_WAV_SEL2
U26.V23 
*SIGNAL* $$$13703
R63.1 U32.8 U32.9 C114.1 
*SIGNAL* $$$26435
C21.2 Y2.1 U26.A23 
*SIGNAL* $$$26436
C22.2 Y2.3 U26.B24 
*SIGNAL* $$$25419
C84.2 L14.1 U31.13 
*SIGNAL* $$$25322
C83.1 U30.4 C49.2 L12.1 
*SIGNAL* $$$26511
C95.2 U37.1 C39.1 L19.1 
*SIGNAL* +3.3V_PZT_TX
U22.1 C65.2 L14.2 R73.1 R63.2 
L32.2 C104.1 C47.1 L16.2 
*SIGNAL* $$$19431
U32.2 L13.2 
*SIGNAL* $$$19433
L15.2 C86.1 U32.4 
*SIGNAL* $$$25510
U32.3 L15.1 C85.1 L16.1 L13.1 
C38.1 
*SIGNAL* $$$19894
U32.5 C86.2 D1.C 
*SIGNAL* $$$27698
R66.1 U32.7 
*SIGNAL* PZT_PWR_EN
U26.R1 R65.1 U42.4 C98.1 U41.4 
*SIGNAL* $$$27702
R66.2 U32.6 R67.2 C87.1 
*SIGNAL* $$$2967
C87.2 R67.1 R68.2 
*SIGNAL* $$$3237
R69.2 R70.1 
*SIGNAL* $$$3259
R70.2 R71.1 U32.10 
*SIGNAL* $$$3655
U41.2 L31.1 U41.1 C56.1 
*SIGNAL* +3.3V_PZT_RX
L31.2 C113.1 R90.1 R8.1 R35.2 
C45.1 L1.2 C46.1 L19.2 C50.1 
L20.2 C55.2 
*SIGNAL* +2.75V_CP
U38.11 R72.2 L22.2 C2.2 C7.1 
C44.1 
*SIGNAL* -2.75V_CP
U38.6 R78.1 C5.1 L23.2 C4.2 
C43.1 
*SIGNAL* $$$14934
C96.1 U38.10 
*SIGNAL* $$$14941
C96.2 U38.9 
*SIGNAL* $$$15655
U38.1 R64.2 
*SIGNAL* $$$17850
U38.3 R64.1 L20.1 C10.1 C12.2 
*SIGNAL* $$$16265
R72.1 U38.2 R76.2 
*SIGNAL* $$$16444
U38.7 R81.1 R78.2 
*SIGNAL* $$$16815
C52.1 U38.5 
*SIGNAL* $$$20303
R83.1 R84.2 C103.1 
*SIGNAL* $$$20306
R84.1 C105.1 T3.1 C78.2 
*SIGNAL* \PZT_SPI_CS
U26.AC15 R14.1 
*SIGNAL* $$$22044
R87.1 C106.1 U37.3 T6.1 
*SIGNAL* $$$25374
U33.1 L17.2 C90.1 

*MISC*      MISCELLANEOUS PARAMETERS

*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

LAYER	METRIC
{
LAYER	0
{
LAYER_THICKNESS	0
DIELECTRIC	3.300000
}
LAYER	1
{
LAYER_NAME	Top Component
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ASSOCIATED_SILK_SCREEN	Silkscreen Top
ASSOCIATED_PASTE_MASK	Paste Mask Top
ASSOCIATED_SOLDER_MASK	Solder Mask Top
ASSOCIATED_ASSEMBLY	Assembly Drawing Top
COMPONENT	Y
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0.254
COPPER_THICKNESS	0.03429
DIELECTRIC	4.300000
COST	0
}
LAYER	2
{
LAYER_NAME	Inner Layer 2
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0.254
COPPER_THICKNESS	0.03429
DIELECTRIC	4.300000
COST	0
}
LAYER	3
{
LAYER_NAME	Inner Layer 3
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0.254
COPPER_THICKNESS	0.03429
DIELECTRIC	4.300000
COST	0
}
LAYER	4
{
LAYER_NAME	Bottom Component
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ASSOCIATED_SILK_SCREEN	Silkscreen Bottom
ASSOCIATED_PASTE_MASK	Paste Mask Bottom
ASSOCIATED_SOLDER_MASK	Solder Mask Bottom
ASSOCIATED_ASSEMBLY	Assembly Drawing Bottom
COMPONENT	Y
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0.03429
DIELECTRIC	3.300000
COST	0
}
LAYER	5
{
LAYER_NAME	Layer_5
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
ENABLED	Y
LAYER_THICKNESS	0.254
COPPER_THICKNESS	0.03429
DIELECTRIC	4.300000
COST	0
}
LAYER	6
{
LAYER_NAME	Layer_6
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ASSOCIATED_SILK_SCREEN	Silkscreen Bottom
ASSOCIATED_PASTE_MASK	Paste Mask Bottom
ASSOCIATED_SOLDER_MASK	Solder Mask Bottom
ASSOCIATED_ASSEMBLY	Assembly Drawing Bottom
COMPONENT	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0.03429
DIELECTRIC	3.300000
COST	0
}
LAYER	7
{
LAYER_NAME	Layer_7
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	8
{
LAYER_NAME	Layer_8
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	9
{
LAYER_NAME	Layer_9
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	10
{
LAYER_NAME	Layer_10
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	11
{
LAYER_NAME	Layer_11
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	12
{
LAYER_NAME	Layer_12
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	13
{
LAYER_NAME	Layer_13
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	14
{
LAYER_NAME	Layer_14
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	15
{
LAYER_NAME	Layer_15
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	16
{
LAYER_NAME	Layer_16
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	17
{
LAYER_NAME	Layer_17
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	18
{
LAYER_NAME	Layer_18
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	19
{
LAYER_NAME	Layer_19
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	20
{
LAYER_NAME	Layer_20
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	21
{
LAYER_NAME	Solder Mask Top
LAYER_TYPE	SOLDER_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	22
{
LAYER_NAME	Paste Mask Bottom
LAYER_TYPE	PASTE_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	23
{
LAYER_NAME	Paste Mask Top
LAYER_TYPE	PASTE_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	24
{
LAYER_NAME	Drill Drawing
LAYER_TYPE	DRILL
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	25
{
LAYER_NAME	Layer_25
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	26
{
LAYER_NAME	Silkscreen Top
LAYER_TYPE	SILK_SCREEN
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	27
{
LAYER_NAME	Assembly Drawing Top
LAYER_TYPE	ASSEMBLY
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	28
{
LAYER_NAME	Solder Mask Bottom
LAYER_TYPE	SOLDER_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	29
{
LAYER_NAME	Silkscreen Bottom
LAYER_TYPE	SILK_SCREEN
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	30
{
LAYER_NAME	Assembly Drawing Bottom
LAYER_TYPE	ASSEMBLY
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
}
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

RULES_SECTION	METRIC
{
NET_CLASS	DATA
DESIGN	RULES
{
RULE_SET	(1)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.1
VIA_TO_TRACK	0.1
VIA_TO_VIA	0.1
PAD_TO_TRACK	0.1
PAD_TO_VIA	0.1
PAD_TO_PAD	0.1
SMD_TO_TRACK	0.1
SMD_TO_VIA	0.1
SMD_TO_PAD	0.1
SMD_TO_SMD	0.1
COPPER_TO_TRACK	0.1
COPPER_TO_VIA	0.1
COPPER_TO_PAD	0.1
COPPER_TO_SMD	0.1
COPPER_TO_COPPER	0.1
TEXT_TO_TRACK	0.1
TEXT_TO_VIA	0.1
TEXT_TO_PAD	0.1
TEXT_TO_SMD	0.1
OUTLINE_TO_TRACK	0.2
OUTLINE_TO_VIA	0.2
OUTLINE_TO_PAD	0.2
OUTLINE_TO_SMD	0.2
OUTLINE_TO_COPPER	0.2
DRILL_TO_TRACK	0.1
DRILL_TO_VIA	0.1
DRILL_TO_PAD	0.1
DRILL_TO_SMD	0.1
DRILL_TO_COPPER	0.1
SAME_NET_SMD_TO_VIA	0.1
SAME_NET_SMD_TO_CRN	0.1
SAME_NET_VIA_TO_VIA	0.1
SAME_NET_PAD_TO_CRN	0.1
MIN_TRACK_WIDTH	0.1
REC_TRACK_WIDTH	0.1
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1
BODY_TO_BODY	0.1
SAME_NET_TRACK_TO_CRN	0.1
}
}
RULE_SET	(2)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
ROUTE_RULE	:
{
LENGTH_MINIMIZATION_TYPE	1
TRACE_SHARE	Y
VIA_SHARE	Y
AUTO_ROUTE	Y
RIPUP	Y
SHOVE	Y
ROUTE_PRIORITY	3
MAX_NUMBER_OF_VIAS	-1
VALID_LAYER	1
VALID_LAYER	2
VALID_LAYER	3
VALID_LAYER	4
VALID_VIA_TYPE	MICROVIA
VALID_VIA_TYPE	STANDARDVIA
VALID_VIA_TYPE	NOPLATED
VALID_VIA_TYPE	GUIDEHOLE
}
}
RULE_SET	(3)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
HIGH_SPEED_RULE	:
{
MIN_LENGTH	0
MAX_LENGTH	1269.99996
STUB_LENGTH	0
PARALLEL_LENGTH	25.4
PARALLEL_GAP	5.08
TANDEM_LENGTH	25.4
TANDEM_GAP	5.08
MIN_DELAY	0.000000
MAX_DELAY	10.000000
MIN_CAPACITANCE	0.000000
MAX_CAPACITANCE	10.000000
MIN_IMPEDANCE	50.000000
MAX_IMPEDANCE	150.000000
SHIELD_NET	*
SHIELD_GAP	5.08
MATCH_LENGTH_TOLERANCE	5.08
}
}
RULE_SET	(4)
{
FOR	:
{
NET	VDD_BAT
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.1
VIA_TO_TRACK	0.1
VIA_TO_VIA	0.1
PAD_TO_TRACK	0.1
PAD_TO_VIA	0.1
PAD_TO_PAD	0.1
SMD_TO_TRACK	0.1
SMD_TO_VIA	0.1
SMD_TO_PAD	0.1
SMD_TO_SMD	0.1
COPPER_TO_TRACK	0.1
COPPER_TO_VIA	0.1
COPPER_TO_PAD	0.1
COPPER_TO_SMD	0.1
COPPER_TO_COPPER	0.1
TEXT_TO_TRACK	0.1
TEXT_TO_VIA	0.1
TEXT_TO_PAD	0.1
TEXT_TO_SMD	0.1
OUTLINE_TO_TRACK	0.15
OUTLINE_TO_VIA	0.15
OUTLINE_TO_PAD	0.15
OUTLINE_TO_SMD	0.15
OUTLINE_TO_COPPER	0.15
DRILL_TO_TRACK	0.1
DRILL_TO_VIA	0.1
DRILL_TO_PAD	0.1
DRILL_TO_SMD	0.1
DRILL_TO_COPPER	0.1
SAME_NET_SMD_TO_VIA	0.1
SAME_NET_SMD_TO_CRN	0.1
SAME_NET_VIA_TO_VIA	0.1
SAME_NET_PAD_TO_CRN	0.1
MIN_TRACK_WIDTH	0.1
REC_TRACK_WIDTH	0.2
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1
BODY_TO_BODY	0.1
SAME_NET_TRACK_TO_CRN	0.1
}
}
RULE_SET	(5)
{
FOR	:
{
NET	ANT
NET	$$$16529
NET	$$$3606
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.1
VIA_TO_TRACK	0.1
VIA_TO_VIA	0.1
PAD_TO_TRACK	0.1
PAD_TO_VIA	0.1
PAD_TO_PAD	0.1
SMD_TO_TRACK	0.1
SMD_TO_VIA	0.1
SMD_TO_PAD	0.1
SMD_TO_SMD	0.1
COPPER_TO_TRACK	0.1
COPPER_TO_VIA	0.1
COPPER_TO_PAD	0.1
COPPER_TO_SMD	0.1
COPPER_TO_COPPER	0.1
TEXT_TO_TRACK	0.1
TEXT_TO_VIA	0.1
TEXT_TO_PAD	0.1
TEXT_TO_SMD	0.1
OUTLINE_TO_TRACK	0.2
OUTLINE_TO_VIA	0.2
OUTLINE_TO_PAD	0.2
OUTLINE_TO_SMD	0.2
OUTLINE_TO_COPPER	0.2
DRILL_TO_TRACK	0.1
DRILL_TO_VIA	0.1
DRILL_TO_PAD	0.1
DRILL_TO_SMD	0.1
DRILL_TO_COPPER	0.1
SAME_NET_SMD_TO_VIA	0.1
SAME_NET_SMD_TO_CRN	0.1
SAME_NET_VIA_TO_VIA	0.1
SAME_NET_PAD_TO_CRN	0.1
MIN_TRACK_WIDTH	0.1
REC_TRACK_WIDTH	0.3
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1
BODY_TO_BODY	0.1
SAME_NET_TRACK_TO_CRN	0.1
}
}
RULE_SET	(6)
{
FOR	:
{
NET	+3.3V_M
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.1
VIA_TO_TRACK	0.1
VIA_TO_VIA	0.1
PAD_TO_TRACK	0.1
PAD_TO_VIA	0.1
PAD_TO_PAD	0.1
SMD_TO_TRACK	0.1
SMD_TO_VIA	0.1
SMD_TO_PAD	0.1
SMD_TO_SMD	0.1
COPPER_TO_TRACK	0.1
COPPER_TO_VIA	0.1
COPPER_TO_PAD	0.1
COPPER_TO_SMD	0.1
COPPER_TO_COPPER	0.1
TEXT_TO_TRACK	0.1
TEXT_TO_VIA	0.1
TEXT_TO_PAD	0.1
TEXT_TO_SMD	0.1
OUTLINE_TO_TRACK	0.2
OUTLINE_TO_VIA	0.2
OUTLINE_TO_PAD	0.2
OUTLINE_TO_SMD	0.2
OUTLINE_TO_COPPER	0.2
DRILL_TO_TRACK	0.1
DRILL_TO_VIA	0.1
DRILL_TO_PAD	0.1
DRILL_TO_SMD	0.1
DRILL_TO_COPPER	0.1
SAME_NET_SMD_TO_VIA	0.1
SAME_NET_SMD_TO_CRN	0.1
SAME_NET_VIA_TO_VIA	0.1
SAME_NET_PAD_TO_CRN	0.1
MIN_TRACK_WIDTH	0.1
REC_TRACK_WIDTH	0.3
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1
BODY_TO_BODY	0.1
SAME_NET_TRACK_TO_CRN	0.1
}
}
RULE_SET	(7)
{
FOR	:
{
NET	GND
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.1
VIA_TO_TRACK	0.1
VIA_TO_VIA	0.1
PAD_TO_TRACK	0.1
PAD_TO_VIA	0.1
PAD_TO_PAD	0.1
SMD_TO_TRACK	0.1
SMD_TO_VIA	0.1
SMD_TO_PAD	0.1
SMD_TO_SMD	0.1
COPPER_TO_TRACK	0.1
COPPER_TO_VIA	0.1
COPPER_TO_PAD	0.1
COPPER_TO_SMD	0.1
COPPER_TO_COPPER	0.1
TEXT_TO_TRACK	0.1
TEXT_TO_VIA	0.1
TEXT_TO_PAD	0.1
TEXT_TO_SMD	0.1
OUTLINE_TO_TRACK	0.2
OUTLINE_TO_VIA	0.2
OUTLINE_TO_PAD	0.2
OUTLINE_TO_SMD	0.2
OUTLINE_TO_COPPER	0.2
DRILL_TO_TRACK	0.1
DRILL_TO_VIA	0.1
DRILL_TO_PAD	0.1
DRILL_TO_SMD	0.1
DRILL_TO_COPPER	0.1
SAME_NET_SMD_TO_VIA	0.1
SAME_NET_SMD_TO_CRN	0.1
SAME_NET_VIA_TO_VIA	0.1
SAME_NET_PAD_TO_CRN	0.1
MIN_TRACK_WIDTH	0.1
REC_TRACK_WIDTH	0.2
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1
BODY_TO_BODY	0.1
SAME_NET_TRACK_TO_CRN	0.1
}
}
RULE_SET	(8)
{
FOR	:
{
NET	ADC_BAT
NET	VDD_BAT
NET	$$$14940
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.1
VIA_TO_TRACK	0.1
VIA_TO_VIA	0.1
PAD_TO_TRACK	0.1
PAD_TO_VIA	0.1
PAD_TO_PAD	0.1
SMD_TO_TRACK	0.1
SMD_TO_VIA	0.1
SMD_TO_PAD	0.1
SMD_TO_SMD	0.1
COPPER_TO_TRACK	0.1
COPPER_TO_VIA	0.1
COPPER_TO_PAD	0.1
COPPER_TO_SMD	0.1
COPPER_TO_COPPER	0.1
TEXT_TO_TRACK	0.1
TEXT_TO_VIA	0.1
TEXT_TO_PAD	0.1
TEXT_TO_SMD	0.1
OUTLINE_TO_TRACK	0.2
OUTLINE_TO_VIA	0.2
OUTLINE_TO_PAD	0.2
OUTLINE_TO_SMD	0.2
OUTLINE_TO_COPPER	0.2
DRILL_TO_TRACK	0.1
DRILL_TO_VIA	0.1
DRILL_TO_PAD	0.1
DRILL_TO_SMD	0.1
DRILL_TO_COPPER	0.1
SAME_NET_SMD_TO_VIA	0.1
SAME_NET_SMD_TO_CRN	0.1
SAME_NET_VIA_TO_VIA	0.1
SAME_NET_PAD_TO_CRN	0.1
MIN_TRACK_WIDTH	0.1
REC_TRACK_WIDTH	0.5
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1
BODY_TO_BODY	0.1
SAME_NET_TRACK_TO_CRN	0.1
}
}
RULE_SET	(9)
{
FOR	:
{
NET	$$$6537
NET	$$$6539
NET	$$$25431
NET	$$$25958
NET	$$$26274
NET	$$$27542
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.1
VIA_TO_TRACK	0.1
VIA_TO_VIA	0.1
PAD_TO_TRACK	0.1
PAD_TO_VIA	0.1
PAD_TO_PAD	0.1
SMD_TO_TRACK	0.1
SMD_TO_VIA	0.1
SMD_TO_PAD	0.1
SMD_TO_SMD	0.1
COPPER_TO_TRACK	0.1
COPPER_TO_VIA	0.1
COPPER_TO_PAD	0.1
COPPER_TO_SMD	0.1
COPPER_TO_COPPER	0.1
TEXT_TO_TRACK	0.1
TEXT_TO_VIA	0.1
TEXT_TO_PAD	0.1
TEXT_TO_SMD	0.1
OUTLINE_TO_TRACK	0.2
OUTLINE_TO_VIA	0.2
OUTLINE_TO_PAD	0.2
OUTLINE_TO_SMD	0.2
OUTLINE_TO_COPPER	0.2
DRILL_TO_TRACK	0.1
DRILL_TO_VIA	0.1
DRILL_TO_PAD	0.1
DRILL_TO_SMD	0.1
DRILL_TO_COPPER	0.1
SAME_NET_SMD_TO_VIA	0.1
SAME_NET_SMD_TO_CRN	0.1
SAME_NET_VIA_TO_VIA	0.1
SAME_NET_PAD_TO_CRN	0.1
MIN_TRACK_WIDTH	0.1
REC_TRACK_WIDTH	0.2
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1
BODY_TO_BODY	0.1
SAME_NET_TRACK_TO_CRN	0.1
}
}
RULE_SET	(10)
{
FOR	:
{
NET	VBUS
NET	$$$12824
NET	\SPI_CS_FLASH
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.1
VIA_TO_TRACK	0.1
VIA_TO_VIA	0.1
PAD_TO_TRACK	0.1
PAD_TO_VIA	0.1
PAD_TO_PAD	0.1
SMD_TO_TRACK	0.1
SMD_TO_VIA	0.1
SMD_TO_PAD	0.1
SMD_TO_SMD	0.1
COPPER_TO_TRACK	0.1
COPPER_TO_VIA	0.1
COPPER_TO_PAD	0.1
COPPER_TO_SMD	0.1
COPPER_TO_COPPER	0.1
TEXT_TO_TRACK	0.1
TEXT_TO_VIA	0.1
TEXT_TO_PAD	0.1
TEXT_TO_SMD	0.1
OUTLINE_TO_TRACK	0.2
OUTLINE_TO_VIA	0.2
OUTLINE_TO_PAD	0.2
OUTLINE_TO_SMD	0.2
OUTLINE_TO_COPPER	0.2
DRILL_TO_TRACK	0.1
DRILL_TO_VIA	0.1
DRILL_TO_PAD	0.1
DRILL_TO_SMD	0.1
DRILL_TO_COPPER	0.1
SAME_NET_SMD_TO_VIA	0.1
SAME_NET_SMD_TO_CRN	0.1
SAME_NET_VIA_TO_VIA	0.1
SAME_NET_PAD_TO_CRN	0.1
MIN_TRACK_WIDTH	0.1
REC_TRACK_WIDTH	0.5
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1
BODY_TO_BODY	0.1
SAME_NET_TRACK_TO_CRN	0.1
}
}
RULE_SET	(11)
{
FOR	:
{
NET	$$$85
NET	$$$1313
NET	$$$1329
NET	$$$24450
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.1
VIA_TO_TRACK	0.1
VIA_TO_VIA	0.1
PAD_TO_TRACK	0.1
PAD_TO_VIA	0.1
PAD_TO_PAD	0.1
SMD_TO_TRACK	0.1
SMD_TO_VIA	0.1
SMD_TO_PAD	0.1
SMD_TO_SMD	0.1
COPPER_TO_TRACK	0.1
COPPER_TO_VIA	0.1
COPPER_TO_PAD	0.1
COPPER_TO_SMD	0.1
COPPER_TO_COPPER	0.1
TEXT_TO_TRACK	0.1
TEXT_TO_VIA	0.1
TEXT_TO_PAD	0.1
TEXT_TO_SMD	0.1
OUTLINE_TO_TRACK	0.2
OUTLINE_TO_VIA	0.2
OUTLINE_TO_PAD	0.2
OUTLINE_TO_SMD	0.2
OUTLINE_TO_COPPER	0.2
DRILL_TO_TRACK	0.1
DRILL_TO_VIA	0.1
DRILL_TO_PAD	0.1
DRILL_TO_SMD	0.1
DRILL_TO_COPPER	0.1
SAME_NET_SMD_TO_VIA	0.1
SAME_NET_SMD_TO_CRN	0.1
SAME_NET_VIA_TO_VIA	0.1
SAME_NET_PAD_TO_CRN	0.1
MIN_TRACK_WIDTH	0.1
REC_TRACK_WIDTH	0.3
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1
BODY_TO_BODY	0.1
SAME_NET_TRACK_TO_CRN	0.1
}
}
RULE_SET	(12)
{
FOR	:
{
NET	VDD_MAIN
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.1
VIA_TO_TRACK	0.1
VIA_TO_VIA	0.1
PAD_TO_TRACK	0.1
PAD_TO_VIA	0.1
PAD_TO_PAD	0.1
SMD_TO_TRACK	0.1
SMD_TO_VIA	0.1
SMD_TO_PAD	0.1
SMD_TO_SMD	0.1
COPPER_TO_TRACK	0.1
COPPER_TO_VIA	0.1
COPPER_TO_PAD	0.1
COPPER_TO_SMD	0.1
COPPER_TO_COPPER	0.1
TEXT_TO_TRACK	0.1
TEXT_TO_VIA	0.1
TEXT_TO_PAD	0.1
TEXT_TO_SMD	0.1
OUTLINE_TO_TRACK	0.2
OUTLINE_TO_VIA	0.2
OUTLINE_TO_PAD	0.2
OUTLINE_TO_SMD	0.2
OUTLINE_TO_COPPER	0.2
DRILL_TO_TRACK	0.1
DRILL_TO_VIA	0.1
DRILL_TO_PAD	0.1
DRILL_TO_SMD	0.1
DRILL_TO_COPPER	0.1
SAME_NET_SMD_TO_VIA	0.1
SAME_NET_SMD_TO_CRN	0.1
SAME_NET_VIA_TO_VIA	0.1
SAME_NET_PAD_TO_CRN	0.1
MIN_TRACK_WIDTH	0.1
REC_TRACK_WIDTH	0.3
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1
BODY_TO_BODY	0.1
SAME_NET_TRACK_TO_CRN	0.1
}
}
RULE_SET	(14)
{
FOR	:
{
NET	ADC_AGC
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.1
VIA_TO_TRACK	0.1
VIA_TO_VIA	0.1
PAD_TO_TRACK	0.1
PAD_TO_VIA	0.1
PAD_TO_PAD	0.1
SMD_TO_TRACK	0.1
SMD_TO_VIA	0.1
SMD_TO_PAD	0.1
SMD_TO_SMD	0.1
COPPER_TO_TRACK	0.1
COPPER_TO_VIA	0.1
COPPER_TO_PAD	0.1
COPPER_TO_SMD	0.1
COPPER_TO_COPPER	0.1
TEXT_TO_TRACK	0.1
TEXT_TO_VIA	0.1
TEXT_TO_PAD	0.1
TEXT_TO_SMD	0.1
OUTLINE_TO_TRACK	0.2
OUTLINE_TO_VIA	0.2
OUTLINE_TO_PAD	0.2
OUTLINE_TO_SMD	0.2
OUTLINE_TO_COPPER	0.2
DRILL_TO_TRACK	0.1
DRILL_TO_VIA	0.1
DRILL_TO_PAD	0.1
DRILL_TO_SMD	0.1
DRILL_TO_COPPER	0.1
SAME_NET_SMD_TO_VIA	0.1
SAME_NET_SMD_TO_CRN	0.1
SAME_NET_VIA_TO_VIA	0.1
SAME_NET_PAD_TO_CRN	0.1
MIN_TRACK_WIDTH	0.1
REC_TRACK_WIDTH	0.3
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1
BODY_TO_BODY	0.1
SAME_NET_TRACK_TO_CRN	0.1
}
}
RULE_SET	(15)
{
FOR	:
{
NET	ADC_RDATA_N
NET	ADC_RDATA_P
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.1
VIA_TO_TRACK	0.1
VIA_TO_VIA	0.1
PAD_TO_TRACK	0.1
PAD_TO_VIA	0.1
PAD_TO_PAD	0.1
SMD_TO_TRACK	0.1
SMD_TO_VIA	0.1
SMD_TO_PAD	0.1
SMD_TO_SMD	0.1
COPPER_TO_TRACK	0.1
COPPER_TO_VIA	0.1
COPPER_TO_PAD	0.1
COPPER_TO_SMD	0.1
COPPER_TO_COPPER	0.1
TEXT_TO_TRACK	0.1
TEXT_TO_VIA	0.1
TEXT_TO_PAD	0.1
TEXT_TO_SMD	0.1
OUTLINE_TO_TRACK	0.2
OUTLINE_TO_VIA	0.2
OUTLINE_TO_PAD	0.2
OUTLINE_TO_SMD	0.2
OUTLINE_TO_COPPER	0.2
DRILL_TO_TRACK	0.1
DRILL_TO_VIA	0.1
DRILL_TO_PAD	0.1
DRILL_TO_SMD	0.1
DRILL_TO_COPPER	0.1
SAME_NET_SMD_TO_VIA	0.1
SAME_NET_SMD_TO_CRN	0.1
SAME_NET_VIA_TO_VIA	0.1
SAME_NET_PAD_TO_CRN	0.1
MIN_TRACK_WIDTH	0.1
REC_TRACK_WIDTH	0.3
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1
BODY_TO_BODY	0.1
SAME_NET_TRACK_TO_CRN	0.1
}
}
}
}

*MISC*      MISCELLANEOUS PARAMETERS

ATTRIBUTE VALUES
{
PART R31
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C17
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 12pF_1005
"Tolerance" 
"Voltage Rating" 
}
PART U2
{
"Manufacturer_Name" Texas Instruments
"Value" OPA2836IDGSR
"Mouser Part Number" 595-OPA2836IDGSR
"Mouser Price/Stock" https://www.mouser.co.uk/ProductDetail/Texas-Instruments/OPA2836IDGSR?qs=RqytGdBYyUGqgkd64C%252BPLQ%3D%3D
"Arrow Part Number" OPA2836IDGSR
"Arrow Price/Stock" https://www.arrow.com/en/products/opa2836idgsr/texas-instruments?utm_currency=USD&region=europe
"Description" Dual, Very Low Power, Rail to Rail out, Negative Rail in, VFB Op Amp
"Datasheet Link" http://www.ti.com/lit/gpn/opa2836
"Geometry.Height" 1.1mm
}
PART C18
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
"Tolerance" 
"Voltage Rating" 
}
PART J2
{
"Description" Battery Connector
"Manufacturer #1" MOLEX
"Value" 2026560021
}
PART R23
{
"Value" 2k_1005_5%
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART R8
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART U9
{
"Manufacturer_Name" Taoglas
"Value" RECE.20279.001E.01
"Mouser Part Number" 960-RECE20279001E01
"Mouser Price/Stock" https://www.mouser.co.uk/ProductDetail/Taoglas/RECE.20279.001E.01?qs=MyNHzdoqoQIdppWb9vcEBA%3D%3D
"Arrow Part Number" RECE.20279.001E.01
"Arrow Price/Stock" https://www.arrow.com/en/products/rece.20279.001e.01/taoglas?utm_currency=USD&region=nac
"Description" IPEX MHF Receptacle
"Datasheet Link" https://datasheet.datasheetarchive.com/originals/distributors/Datasheets-DGA15/760324.pdf
}
PART R11
{
"Value" 0_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C2
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART C30
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART C4
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART R25
{
"Value" 4.7k_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART J4
{
"MF" ATTEND_Technology
"MAXIMUM_PACKAGE_HEIGHT" 5.46_mm
"Package" None
"Price" None
"Check_prices" https://www.snapeda.com/parts/217B-CA04/Attend/view-part/?ref=eda
"STANDARD" Manufacturer_Recommendations
"PARTREV" 1
"SnapEDA_Link" https://www.snapeda.com/parts/217B-CA04/Attend/view-part/?ref=snap
"Value" 217B-CA04
"Description" ______________________________________________________USB-C_(USB_TYPE-C)_Receptacle_Connector_24_(16+8_Dummy)_Position_Surface_Mount,_Right_Angle______________________________________________
"Availability" In_Stock
"MANUFACTURER" Attend
"PKG_TYPE" ATTEND_217B-CA04
}
PART J1
{
"Value" NC
}
PART C19
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 1uF_1005
"Tolerance" 
"Voltage Rating" 
}
PART C16
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 12pF_1005
"Tolerance" 
"Voltage Rating" 
}
PART C23
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 1nF_1005
"Tolerance" 
"Voltage Rating" 
}
PART R28
{
"Value" 806k_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART R42
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R6
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R12
{
"Value" 48.7_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART U5
{
"Description" High Performance 500 mA LDO
"Manufacturer #1" MICROCHIP
"Value" MIC5528-3.3YMT
}
PART C21
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 12pF_1005
"Tolerance" 
"Voltage Rating" 
}
PART C22
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 12pF_1005
"Tolerance" 
"Voltage Rating" 
}
PART C31
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
"Tolerance" 
"Voltage Rating" 
}
PART R14
{
"Value" 0_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART LED3
{
"Description" LED GREEN/1608
"Value" FC-DA1608UGK-520D10
"Manufacturer #1" ANY VENDOR
}
PART C32
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART C20
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
"Tolerance" 
"Voltage Rating" 
}
PART R16
{
"Value" 0_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R18
{
"Value" 0_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART U20
{
"Manufacturer_Name" Nexperia
"Value" PESD5V0F1BLD,315
"Mouser Part Number" 771-PESD5V0F1BLD315
"Mouser Price/Stock" https://www.mouser.co.uk/ProductDetail/Nexperia/PESD5V0F1BLD315?qs=1sbE9T7hb3b3MsEvtkPidA%3D%3D
"Arrow Part Number" PESD5V0F1BLD,315
"Arrow Price/Stock" https://www.arrow.com/en/products/pesd5v0f1bld315/nexperia?region=nac
"Description" PESD5V0F1BLD - Femtofarad bidirectional ESD protection diode
"Datasheet Link" https://assets.nexperia.com/documents/data-sheet/PESD5V0F1BLD.pdf
"Geometry.Height" 0.4mm
}
PART C15
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 47nF_1005
"Tolerance" 
"Voltage Rating" 
}
PART C24
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 820pF_1005
"Tolerance" 
"Voltage Rating" 
}
PART C5
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 10uF_1608
"Tolerance" 
"Voltage Rating" 
}
PART C7
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 10uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART C10
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608
"Tolerance" 
"Voltage Rating" 
}
PART C14
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 1uF_1005
"Tolerance" 
"Voltage Rating" 
}
PART C12
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART C13
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART C37
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART C38
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART U23
{
"Manufacturer_Name" Analog Devices
"Value" ADL5513ACPZ-R7
"Mouser Part Number" 584-ADL5513ACPZ-R7
"Mouser Price/Stock" https://www.mouser.co.uk/ProductDetail/Analog-Devices/ADL5513ACPZ-R7?qs=BpaRKvA4VqGe6%2FPlUcoEpw%3D%3D
"Arrow Part Number" ADL5513ACPZ-R7
"Arrow Price/Stock" https://www.arrow.com/en/products/adl5513acpz-r7/analog-devices?utm_currency=USD&region=nac
"Description" ANALOG DEVICES - ADL5513ACPZ-R7 - DETECTOR, 1MHZ - 4GHZ, 80DB, LFCSP-16
"Datasheet Link" https://www.analog.com/media/en/technical-documentation/data-sheets/ADL5513.pdf
"Geometry.Height" 0.8mm
}
PART C61
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 47nF_1005
}
PART R19
{
"Value" 1k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R29
{
"Value" 2M_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART C64
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100pF_1005
}
PART C67
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 47nF_1005
}
PART R20
{
"Value" 0_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C72
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 100pF_1005
"Tolerance" 
"Voltage Rating" 
}
PART C29
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART L4
{
"Manufacturer #1" TAIYO YUDEN
"Value" 10uH_1608
"Description" RF INDUCTOR
"Part Number" LBMF1608T100K
}
PART L3
{
"Manufacturer #1" TAIYO YUDEN
"Value" 15nH_1005
"Description" RF INDUCTOR
"Part Number" HK100515NJ-T
}
PART Y1
{
"Cost" 
"Description" CRYSTAL FC-12M 32.768KHZ   20PPM,12.5PF
"Manufacturer #1" SEIKO EPSON
"Value" FC-12M 32.7680KA-A0
"Geometry.Height" 1.27000mm
}
PART R26
{
"Value" NC
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R27
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART Y2
{
"Value" FA-128 32.0000MF10Z-AJ0
"Manufacturer #1" SEIKO EPSON
"Cost" 
"Description" CRYSTAL 2016 32MHz, 8PF(6PF),   10PPM
}
PART R35
{
"Value" 100k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C51
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART L1
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART C42
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART C36
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
"Tolerance" 
"Voltage Rating" 
}
PART R24
{
"Value" 4.7k_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART C43
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 10uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART C39
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART C28
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" NC
"Tolerance" 
"Voltage Rating" 
}
PART C27
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" NC
"Tolerance" 
}
PART R36
{
"Value" 1k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C26
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 0.5pF_1005
"Tolerance" 
"Voltage Rating" 
}
PART C25
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 0.8pF_1005
"Tolerance" 
"Voltage Rating" 
}
PART R39
{
"Value" 1k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C40
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100pF_1005
}
PART C41
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 47pF_1005
}
PART C44
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 10uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART C45
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 10uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART C46
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 10uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART C47
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 10uF_1608
"Tolerance" 
"Voltage Rating" 
}
PART C48
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 1uF_1005_50V
}
PART C49
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 1uF_1005_50V
}
PART U16
{
"Manufacturer_Name" Winbond
"Value" W25Q32RVXHJQ TR
"Mouser Part Number" 454-W25Q32RVXHJQTR
"Mouser Price/Stock" https://www.mouser.co.uk/ProductDetail/Winbond/W25Q32RVXHJQ-TR?qs=mELouGlnn3dFwM4lg8JCig%3D%3D
"Arrow Part Number" W25Q32RVXHJQ TR
"Arrow Price/Stock" https://www.arrow.com/en/products/w25q32rvxhjq-tr/winbond-electronics?utm_currency=USD&region=nac
"Description" NOR Flash spiFlash, 3V, 32M-bit, 4Kb Uniform Sector
"Datasheet Link" https://www.winbond.com/hq/product/code-storage-flash-memory/serial-nor-flash/?__locale=ja&partNo=W25Q32RV
"Geometry.Height" 0.4mm
}
PART C50
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 10uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART C103
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100pF_1005
}
PART R83
{
"Value" 1k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C52
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608
"Tolerance" 
"Voltage Rating" 
}
PART R30
{
"Value" 48.7_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C34
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
"Tolerance" 
"Voltage Rating" 
}
PART R40
{
"Value" 48.7_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART L5
{
"Manufacturer #1" MURATA
"Value" 4.7nH_1005
"Description" RF INDUCTOR
"Part Number" LQP15MN3N9B02D
}
PART U6
{
"MF" Murata
"MAXIMUM_PACKAGE_HEIGHT" 0.95mm
"Package" 1608_Taiyo_Yuden
"Price" None
"Check_prices" https://www.snapeda.com/parts/PRG18BC1R0MM1RB/Murata/view-part/?ref=eda
"STANDARD" IPC-7351B
"PARTREV" N/A
"SnapEDA_Link" https://www.snapeda.com/parts/PRG18BC1R0MM1RB/Murata/view-part/?ref=snap
"Value" PRG18BC1R0MM1RB
"Description" ______________________________________________________Ceramic_PTC_Resettable_Fuse_6V_330_mA_Ih_Surface_Mount_0603_(1608_Metric)______________________________________________
"Availability" In_Stock
"MANUFACTURER" Murata
"PKG_TYPE" THRMC1608X95N
}
PART U7
{
"MF" Murata
"MAXIMUM_PACKAGE_HEIGHT" 0.95mm
"Package" 1608_Taiyo_Yuden
"Price" None
"Check_prices" https://www.snapeda.com/parts/PRG18BC1R0MM1RB/Murata/view-part/?ref=eda
"STANDARD" IPC-7351B
"PARTREV" N/A
"SnapEDA_Link" https://www.snapeda.com/parts/PRG18BC1R0MM1RB/Murata/view-part/?ref=snap
"Value" PRG18BC1R0MM1RB
"Description" ______________________________________________________Ceramic_PTC_Resettable_Fuse_6V_330_mA_Ih_Surface_Mount_0603_(1608_Metric)______________________________________________
"Availability" In_Stock
"MANUFACTURER" Murata
"PKG_TYPE" THRMC1608X95N
}
PART L6
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART SW2
{
"Value" NW3-A03-05
"Manufacturer #1" MADE IN CHINA
"Description" TACTILE SWITCH
}
PART C53
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
"Tolerance" 
"Voltage Rating" 
}
PART R17
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R41
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C54
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART C55
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART C56
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 10uF_1608
"Tolerance" 
"Voltage Rating" 
}
PART R43
{
"Value" 2k_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART LED4
{
"Description" LED ORANGE/1608
"Value" FC-DA1608HOK-600H
"Manufacturer #1" ANY VENDOR
}
PART U4
{
"Manufacturer #1" NEXPERIA
"Value" PMFPB8032XP
"Description" 20V, 3.7A P-channel MOSFET-Schottky
}
PART P1
{
"MANUFACTURER" Panasonic
"PKG_TYPE" PANASONIC_AXT510124
}
PART R15
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART U10
{
"Description" 6-Axis MotionTracking IMU
"Manufacturer #1" TDK_INVENSENSE
"Value" ICM-42670-P
}
PART U27
{
"Manufacturer_Name" Microchip
"Value" MD1822K6-G
"Mouser Part Number" 689-MD1822K6-G
"Mouser Price/Stock" https://www.mouser.co.uk/ProductDetail/Microchip-Technology/MD1822K6-G?qs=SPVxp5Gxk7pFYhy0Y%2FNrig%3D%3D
"Arrow Part Number" MD1822K6-G
"Arrow Price/Stock" https://www.arrow.com/en/products/md1822k6-g/microchip-technology?region=nac
"Description" MICROCHIP - MD1822K6-G - MOSFET Driver, High Side and Low Side, 5V to 10V Supply, 2A Out, 6.5ns Delay, QFN-16
"Datasheet Link" https://ms.componentsearchengine.com/Datasheets/2/MD1822K6-G.pdf
"Geometry.Height" 1mm
}
PART C35
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
"Tolerance" 
"Voltage Rating" 
}
PART C8
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 2.2uF_1608
"Tolerance" 
"Voltage Rating" 
}
PART C9
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART JP1
{
"Value" NC
}
PART R65
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART D3
{
"Description" DUAL SWITCHING DIODE
"Cost" 
"Value" DAP222WM
"Manufacturer #1" ROHM KOREA.
}
PART D4
{
"Description" Medium Power AF Schottky Diode
"Manufacturer #1" INFINEON
"Value" BAS3005B-02V
}
PART U1
{
"Description" ESD protection diode
"Manufacturer #1" NEXPERIA
"Value" PRTR5V0U2X
}
PART R34
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART U22
{
"Description" High-Accuracy Analog Temperature Sensors
"Manufacturer #1" TI
"Value" TMP235AEDBZTQ1
}
PART L2
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART R21
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R22
{
"Value" 100_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART U8
{
"Description" Single Inverter Gate
"Manufacturer #1" TI
"Value" SN74LVC1G04DRY2
}
PART R33
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R32
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R37
{
"Value" 5.1K_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART R4
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART U30
{
"Manufacturer_Name" Microchip
"Value" TC7920K6-G
"Mouser Part Number" 689-TC7920K6-G
"Mouser Price/Stock" https://www.mouser.co.uk/ProductDetail/Microchip-Technology/TC7920K6-G?qs=SPVxp5Gxk7rlZ7Pl2YwJVQ%3D%3D
"Arrow Part Number" TC7920K6-G
"Arrow Price/Stock" https://www.arrow.com/en/products/tc7920k6-g/microchip-technology
"Description" MOSFET 2PR N- & PCH ENHANCE MD MSFET w/DRAIN-DI
"Datasheet Link" https://4donline.ihs.com/images/VipMasterIC/IC/MCHP/MCHP-S-A0019419833/MCHP-S-A0019419833-1.pdf?hkey=EF798316E3902B6ED9A73243A3159BB0
"Geometry.Height" 1mm
}
PART R38
{
"Value" 5.1K_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART C62
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 10nF_1005_50V
}
PART C65
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
"Tolerance" 
"Voltage Rating" 
}
PART C70
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 10nF_1005_50V
}
PART C74
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 10nF_1005_50V
}
PART U26
{
"Copyright" Copyright (C) 2025 Ultra Librarian. All rights reserved.
"Manufacturer_Name" Nordic Semiconductor
"Value" NRF52840-QIAA-F-R
}
PART U3
{
"Description" Advanced Stand-Alone Li-Ion/Li-Polymer Battery Charger
"Manufacturer #1" MICROCHIP
"Value" MCP73838-FCI/UN
}
PART C73
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" NC
"Tolerance" 
"Voltage Rating" 
}
PART C11
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 2.2uF_1608
"Tolerance" 
"Voltage Rating" 
}
PART C75
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 10nF_1005_50V
}
PART U31
{
"Manufacturer_Name" Analog Devices
"Value" MAX14778ETP+
"Mouser Part Number" 700-MAX14778ETP+
"Mouser Price/Stock" https://www.mouser.co.uk/ProductDetail/Analog-Devices-Maxim-Integrated/MAX14778ETP%2b?qs=4Rc5iGDDRGhnkuxvUsFiYQ%3D%3D
"Arrow Part Number" MAX14778ETP+
"Arrow Price/Stock" https://www.arrow.com/en/products/max14778etp/analog-devices?utm_currency=USD&region=nac
"Description" Maxim MAX14778ETP+, Multiplexer Dual 4:1 20Mbit/s, 3  5.5 V, 20-Pin TQFN
"Datasheet Link" https://datasheets.maximintegrated.com/en/ds/MAX14778.pdf
"Geometry.Height" 0.8mm
}
PART C76
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005_50V
}
PART C77
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005_50V
}
PART R58
{
"Value" 0_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C33
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 2.2uF_1608
"Tolerance" 
"Voltage Rating" 
}
PART R73
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R63
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART U34
{
"Value" MD0100N8-G
}
PART C80
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 1uF_1005_50V
}
PART C81
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 1uF_1005_50V
}
PART C82
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005_50V
}
PART C83
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005_50V
}
PART C84
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005_50V
}
PART L10
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART L11
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART L12
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART L14
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART C1
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART U32
{
"MF" Analog_Devices
"VENDOR" Linear_Technology
"Description" ______________________________________________________Boost,_Charge_Pump_Switching_Regulator_IC_Positive_and_Negative_(Dual_Rail)_Adjustable_±1.25V_2_Output_180mA_(Switch),_320mA_(Switch)_10-WFDFN_Exposed_Pad______________________________________________
"Package" DFN-10_Linear_Technology
"Price" None
"Check_prices" https://www.snapeda.com/parts/LT3463EDD%23PBF/Analog+Devices/view-part/?ref=eda
"SnapEDA_Link" https://www.snapeda.com/parts/LT3463EDD%23PBF/Analog+Devices/view-part/?ref=snap
"Value" LT3463EDD#PBF
"Availability" In_Stock
"MANUFACTURER_PART_NUMBER" lt3463edd
"PKG_TYPE" DFN-10_DD
}
PART C3
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART C6
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608_25V
"Tolerance" 
"Voltage Rating" 
}
PART R7
{
"Value" 4.7k_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART L13
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" 10uH_1608
}
PART R10
{
"Value" NC
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART R9
{
"Value" 1.54k_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART R5
{
"Value" 1k_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART L15
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" 10uH_1608
}
PART TH1
{
"Manufacturer #1" KYOCERA AVX
"Value" NB21K00103KBB
"Description" THERMISTOR NTC, 10K/1608
}
PART R13
{
"Value" 69.8k_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART C85
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART C86
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005_50V
}
PART D1
{
"MAXIMUM_PACKAGE_HEIGHT" 1.15mm
"Value" B0540WS
}
PART R66
{
"Value" 61.9k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R67
{
"Value" 1M_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C87
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" NC
}
PART R68
{
"Value" 240k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R69
{
"Value" 240k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R70
{
"Value" 1M_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R71
{
"Value" 66.5k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C88
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 470nF_1005_50V
}
PART C89
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 470nF_1005_50V
}
PART C79
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 1uF_1005
}
PART L16
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART U33
{
"Manufacturer_Name" Microchip
"Value" MCP1804T-A002I/OT
"Mouser Part Number" 579-MCP1804T-A002IOT
"Mouser Price/Stock" https://www.mouser.co.uk/ProductDetail/Microchip-Technology/MCP1804T-A002I-OT?qs=X8nz4ozed5igIlf9%252BFEUbg%3D%3D
"Arrow Part Number" MCP1804T-A002I/OT
"Arrow Price/Stock" https://www.arrow.com/en/products/mcp1804t-a002iot/microchip-technology?region=nac
"Description" LDO, 150mA max, Vin 28V max, Vout =10.0V
"Datasheet Link" http://ww1.microchip.com/downloads/en/DeviceDoc/20002200D.pdf
"Geometry.Height" 1.45mm
}
PART C90
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 1uF_1005_50V
}
PART C91
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 1uF_1005_50V
}
PART C98
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART R1
{
"Value" 1k_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART R2
{
"Value" 1k_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART LED1
{
"Description" LED ORANGE/1608
"Value" FC-DA1608HOK-600H
"Manufacturer #1" ANY VENDOR
}
PART LED2
{
"Description" LED BLUE/1608
"Value" LS-SP192DNB74-D
"Manufacturer #1" ANY VENDOR
}
PART L17
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART R3
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R74
{
"Value" 100k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C110
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 10nF_1005
}
PART R77
{
"Value" 1k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C119
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 10nF_1005
"Tolerance" 
"Voltage Rating" 
}
PART R79
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R80
{
"Value" 100k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART U37
{
"Manufacturer_Name" Texas Instruments
"Value" ADC121S051CIMF/NOPB
"Mouser Part Number" 926-AD121S051CIMFNPB
"Mouser Price/Stock" https://www.mouser.co.uk/ProductDetail/Texas-Instruments/ADC121S051CIMF-NOPB?qs=7X5t%252BdzoRHDM6gt6xt2J%252Bw%3D%3D
"Arrow Part Number" ADC121S051CIMF/NOPB
"Arrow Price/Stock" https://www.arrow.com/en/products/adc121s051cimfnopb/texas-instruments?region=nac
"Description" Single Channel, 200 to 500 ksps, 12-Bit A/D Converter
"Datasheet Link" http://www.ti.com/lit/ds/symlink/adc121s051.pdf
"Geometry.Height" 1.45mm
}
PART C78
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART C93
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART C95
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART L19
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART U38
{
"Manufacturer_Name" Texas Instruments
"Value" LM27762DSSR
"Mouser Part Number" 595-LM27762DSSR
"Mouser Price/Stock" https://www.mouser.co.uk/ProductDetail/Texas-Instruments/LM27762DSSR?qs=vcbl%252BK4rRlfEJcC9xQ80sA%3D%3D
"Arrow Part Number" LM27762DSSR
"Arrow Price/Stock" https://www.arrow.com/en/products/lm27762dssr/texas-instruments?utm_currency=USD&region=nac
"Description" LDO Voltage Regulators Low-Noise Positive- and Negative-Output Integrated Switched Capacitor Plus LDO 12-WSON -40 to 85
"Datasheet Link" https://www.ti.com/lit/ds/symlink/lm27762.pdf
"Geometry.Height" 0.8mm
}
PART U42
{
"Description" High Performance 500 mA LDO
"Manufacturer #1" MICROCHIP
"Value" MIC5528-3.3YMT
}
PART C96
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 1uF_1005
}
PART R64
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R72
{
"Value" 13k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R76
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R78
{
"Value" 13k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART R81
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART L20
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART R82
{
"Value" 1k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART L22
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART L23
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART C102
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART U41
{
"Description" High Performance 500 mA LDO
"Manufacturer #1" MICROCHIP
"Value" MIC5528-3.3YMT
}
PART C104
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 2.2uF_1608
"Tolerance" 
"Voltage Rating" 
}
PART L32
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART R61
{
"Value" 100_1005
"Manufacturer #1" ANY VENDOR
"Part Number" 
"Description" SMT RESISTOR 1005, 1/16W
"Tolerance" 
}
PART C121
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
"Tolerance" 
"Voltage Rating" 
}
PART R84
{
"Value" 1k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C105
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 47pF_1005
}
PART R87
{
"Value" 1.54k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C106
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100pF_1005
}
PART R90
{
"Value" 10k_1005
"Manufacturer #1" ANY VENDOR
"Description" SMT RESISTOR 1005, 1/16W
}
PART C109
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART C113
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 4.7uF_1608
"Tolerance" 
"Voltage Rating" 
}
PART L31
{
"Manufacturer #1" MURATA
"Description" CHIP FERRITE BEAD 120R/2A/1608
"Value" BLM18PG330SH1D
}
PART C114
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Manufacturer #1" ANY VENDOR
"Value" 100nF_1005
}
PART C115
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 2.2uF_1608
"Tolerance" 
"Voltage Rating" 
}
PART C116
{
"Description" SURFACE MOUNT CAPACITOR 1005
"Part Number" 
"Manufacturer #1" ANY VENDOR
"Value" 10uF_1608
"Tolerance" 
"Voltage Rating" 
}
}

*END*     OF ASCII OUTPUT FILE
